{"text_format":"2","workbook":"xlsx","n_sheets":4,"sheets":["通道明细表","模块接口参数","3种屏","终端机"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"通道明细表","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[]}
["单片机接口","硬件名称","名称解析","功能","硬件位置","硬件信息参考文档"]
["电源(V+/V-给单片机板子供电)"]
["V"]
["以太网接口(网口)"]
["LAN1","终端","停车终端（终端连接）"]
["LAN2","号牌机","号牌机licenseNumber","识别车牌号","库内停车区域前端","号牌机资料文档"]
["RS485/232接口（TX/RX）"]
["RS485","地磁接收器","地磁接收器","接收地磁感应信号：检测门外是否有车","库外入口处","地磁接收器通讯协议文档"]
["数字量输入通道（DI）"]
["DI1","光电开关-发射器、接收器","停车超前光电overLimit/front","检测车辆停放位置是否超前","库内停车区域前端","楚天传感器样品说明/开关量通信-输入信号/巴鲁夫光电开关-发射器、接收器.pdf"]
["DI2","光电开关-发射器、接收器","停车超后光电overLimit/back","检测车辆停放位置是否超后","库内停车区域后侧","楚天传感器样品说明/开关量通信-输入信号/巴鲁夫光电开关-发射器、接收器.pdf"]
["DI3","光电开关-发射器、接收器","停车超左光电overLimit/left","检测车辆停放位置是否偏左","库内停车区域左侧","楚天传感器样品说明/开关量通信-输入信号/巴鲁夫光电开关-发射器、接收器.pdf"]
["DI4","光电开关-发射器、接收器","停车超右光电overLimit/right","检测车辆停放位置是否偏右","库内停车区域右侧","楚天传感器样品说明/开关量通信-输入信号/巴鲁夫光电开关-发射器、接收器.pdf"]
["DI5","光电开关-发射器、接收器","停车超高光电overLimit/high","检测入库车辆是否超高","库门顶部","楚天传感器样品说明/开关量通信-输入信号/巴鲁夫光电开关-发射器、接收器.pdf"]
["DI6","光电开关-发射器、接收器","底盘超高信号overLimit/low","检测入库车辆底盘是否过低","库内地面","楚天传感器样品说明/开关量通信-输入信号/巴鲁夫光电开关-发射器、接收器.pdf"]
["DI7","地磁","停车库外地磁geomag/outdoor","检测门外是否有车（发送信号给接收器（无线信号））","库外入口处","楚天传感器样品说明/武汉恒达地磁基站产品介绍.docx"]
["DI8","地感","停车库内地感groundSense/indoor","检测库内是否有车（不需要接收器，地感模块继电器输出（有线信号））","库内地面","楚天传感器样品说明/单双路地感模块参数说明_20200806094907.jpg    研华数字量输入、继电器输出模块参考资料"]
["DI9","外门","停车库门开到位doorState","库门控制盒输出信号","库内门立柱旁","厂家-阔福门"]
["DI10","外门","停车库门关到位doorState","库门控制盒输出信号","库内门立柱旁","厂家-阔福门"]
["DI11","外门","停车库门运行中doorState","库门控制盒输出信号","库内门立柱旁","厂家-阔福门"]
["DI12","外门","停车库门报警doorState","库门控制盒输出信号","库内门立柱旁","厂家-阔福门"]
["DI13","光电开关-发射器、接收器","停车类型光电开关判断suvCar","检测入库车辆高度是否为SUV","库门侧中部","楚天传感器样品说明/开关量通信-输入信号/巴鲁夫光电开关-发射器、接收器.pdf"]
["DI14",null,"备用"]
["DI15",null,"备用"]
["DI16",null,"备用"]
["继电器输出通道（RO）"]
["RO1","外门","开门信号doorControl","库门控制盒接收信号","库内门立柱旁","厂家-阔福门"]
["RO2","外门","关门信号doorControl","库门控制盒接收信号","库内门立柱旁","厂家-阔福门"]
["RO3","外门","停止信号doorControl","库门控制盒接收信号","库内门立柱旁","厂家-阔福门"]
["RO4",null,"备用"]
["RO5",null,"备用"]
["RO6",null,"备用"]
["RO7",null,"备用"]
["RO8",null,"备用"]
["模拟量输入通道（AI）"]
["AI1",null,"备用"]
["AI2",null,"备用"]
["AI3",null,"备用"]
["AI4",null,"备用"]
["模拟量输出通道（AO）"]
["AO1",null,"备用"]
["AO2",null,"备用"]
["AO3",null,"备用"]
["AO4",null,"备用"]
[]
[]
[]
["A/B?可能是板子给传感器供电"]

{"sheet":"模块接口参数","index":1,"n_rows":55,"n_cols":2,"rows_kept":55,"cut":false,"hidden":false,"merged":[]}
[]
["LED显示"]
["电源指示灯","power 绿色代表正常 "]
["状态显示灯","R"]
["通讯指示灯","R"]
["通道指示灯","R"]
["电源"]
["输入电压","10-30VDC(24V DC STANDARD)"]
["输入电源短路保护","R"]
["双电源通道","R"]
["以太网接口","Ethernet"]
["通道数量","2-port"]
["接口类型","RJ45，10/100M Base-TX"]
["通讯协议","TCP/IP"]
["串口通讯接口"]
[485,"逻辑电平+2~+6V代表逻辑“1”，-2~-6V代表逻辑“0”"]
["数字量输入通道","DI"]
["通道数量","16-Chinel"]
["输入电压","干接点：逻辑0：开路；逻辑1：通路；湿节点：逻辑0：0 ~3 VDC；逻辑 1：10~30VDC；"]
["输入频率","0.1~3KHz"]
["干接点","逻辑电平0：开路；逻辑电平1：通路；"]
["湿接点","逻辑 0: 0 ~ 3 VDC 逻辑 1: 10 ~ 30 VDC (干接点/湿接点转换通过微动开关）"]
["输入阻抗","5.2KW（湿接点）"]
["继电器输出通道","Realy output"]
["损毁电压","500V AC(50/60)Hz"]
["通道数量","8-Chinel"]
["触点容量","250 VAC @ 5A 30 VDC @ 5A"]
["操作频率","360 operations/hour with load, 72,000 operations/hour without load"]
["绝缘电阻","> 10 GΩ @ 500 VDC"]
["隔离接触","1000 Vrms"]
["最大损毁容量","1250 VA"]
["最大开关电压","400 VAC, 300 VDC"]
["设置/复位时间","8 ms/8 ms"]
["模拟量输入通道","Analog InPut"]
["精确度","Voltage mode : ±0.1% or better Current mode : ±0.2% or better"]
["通道数量","4 (differential, each channel can be configured with different range)"]
["CMR @ 50/60 Hz","92 dB min"]
["输入阻抗","Voltage: 800K Ω Current: 120 Ω (Build-in 120 Ω. resistor for Current Input) for Current Input)"]
["输入范围","0 ~ 150 mV, 0 ~ 500 mV, 0 ~ 1 V, 0 ~ 5 V, 0 ~ 10 V, 0 ~ 15 V, 4 ~ 20 mA"]
["分辨率","16-bit"]
["抽样率","10 samples/sec. (total)"]
["量程飘移","±25 ppm/°C"]
["零点飘移","±6 μV/°C"]
["高共模","200 VDC"]
["模拟量输出通道","Analog Output"]
["分辨率","±0.1% of FSR for current output ±0.2% of FSR for voltage output"]
["通道数量","4-Chinel"]
["电流负荷","0 ~ 500 Ω (source)"]
["输出类型","mA, V"]
["输出范围","0 ~ 20 mA, 4 ~ 20 mA, 0 ~10 V"]
["可编程输出斜率","0.125 ~ 128.0 mA/sec.  0.0625 ~ 64.0 V/sec."]
["分辨率","12-bit"]
["分辨率","±0.015% of FSR"]
["跨度温度系数","±25 PPM/°C"]
["零点漂移","Voltage: ±30 µV/°C Current: ±0.2 µA/°C"]

{"sheet":"3种屏","index":2,"n_rows":9,"n_cols":12,"rows_kept":9,"cut":false,"hidden":false,"merged":[]}
[]
[null,null,"数量","功能",null,"信号线","电源线","尺寸","重量","安装","厂家信息","备注"]
[null,"入口外LED屏","6个","文字显示入口的状态",null,"超5类网线,对接终端机的局域网","220V",null,null,"入口外门外面上方"]
[]
[]
[null,"出口外LED屏","1个","文字提示用户在指定的出口取车, 以及代取汽车状态",null,"超5类网线,对接终端机的局域网","220V",null,null,"出口外门外面上方"]
[]
[]
[null,"入口内液晶显示屏",null,"图像显示汽车的方位,辅助司机正确停车",null,"HDMI,对接终端机","220V",null,null,"入口门内右前方,或者贴在入口内门上面"]

{"sheet":"终端机","index":3,"n_rows":12,"n_cols":12,"rows_kept":12,"cut":false,"hidden":false,"merged":[[2,1,4,1],[2,2,4,2],[2,3,4,3],[2,6,4,6],[2,9,4,9],[7,1,8,1],[7,2,8,2],[7,3,8,3],[7,9,8,9]]}
[]
[null,null,"数量","功能",null,"信号线","电源线","尺寸","重量","安装","厂家信息","备注"]
[null,"终端机(window电脑)","6个","和用户交互,负责存取车",null,"超5类网线,对接主控的局域网","220V",null,null,"入口外门外面,挂在立柱上或者挂在墙壁上"]
[{"$nulls":5},"超5类网线,直连入口单片机"]
[{"$nulls":5},"HDMI, 对接入口内液晶显示屏"]
[]
[]
[null,"入口单片机","6个","出入口硬件管理,测控入口的所有硬件设备,(门控,地感,光电传感器等等)",null,"超5类网线,直连终端机","220V",null,null,"终端机旁边"]
[{"$nulls":5},"超5类网线,直连号牌机","220V"]
[]
[]
[null,"号牌机","6个","获取车牌号",null,"超5类网线,对入口单片机","220V",null,null,"入口内部左前方或右前方"]