{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":11,"n_cols":8,"rows_kept":11,"cut":false,"hidden":false,"merged":[[4,3,5,4],[4,5,5,6],[4,7,5,8],[2,0,3,8],[4,0,5,0],[6,0,7,0],[4,1,5,2],[8,0,10,0],[8,1,10,2],[6,1,7,2],[6,3,7,4],[8,3,10,4],[6,7,7,8],[6,5,7,6],[8,5,8,6],[9,5,9,6],[8,7,8,8],[9,7,9,8],[10,5,10,6],[10,7,10,8]]}
[]
[]
["楚天测量常见问题汇总"]
[]
["序号","常见问题",null,"问题现象",null,"问题原因",null,"解决办法"]
[]
[1,"雷达掉线",null,"测量命令行界面黄色提示“检测到入口x点云缺失”等字样",null,"激光雷达未上电或网络异常",null,"检查相关网线接头，入口激光雷达断电，30s后重新上电；仍未恢复则联系维护人员。"]
[]
[2,"测量功能异常",null,"停车点击终端后提示测量失败",null,"存在障碍物",null,"清除车辆周边与雷达周边杂物"]
[{"$nulls":5},"激光雷达工作异常",null,"用拭镜纸清理入口激光雷达表面。仍未解决则将入口激光雷达断电，30s后重新上电；仍未恢复则联系维护人员。"]
[{"$nulls":5},"测量软件工作异常，通常此时所有入口均无法正常停车",null,"待无停取车流程时，一键关闭主控所有软件，5s后一键开启"]