{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":74,"n_cols":4,"rows_kept":74,"cut":false,"hidden":false,"merged":[]}
["IP地址","设备类型","设备编号","备注"]
["192.168.1.1",null,null,"通常作为网关，尽量不要分配设备到该ip"]
[]
["192.168.1.120","入口单片机",1,"入口单片机接入局域网，范围120-129"]
["192.168.1.121",null,2]
["192.168.1.122",null,3]
["192.168.1.123",null,4]
["192.168.1.124",null,5]
["192.168.1.125",null,6]
[]
["192.168.1.130","出口单片机",1,"出口单片机接入局域网，范围130-139"]
["192.168.1.131",null,2]
["192.168.1.132",null,3]
["192.168.1.133",null,4]
["192.168.1.134",null,5]
["192.168.1.135",null,6]
[]
["192.168.1.140","入口车头监控相机",1,"目前6个车头相机ip区域140-149，剩余备用"]
["192.168.1.141",null,2]
["192.168.1.142",null,3]
["192.168.1.143",null,4]
["192.168.1.144",null,5]
["192.168.1.145",null,6]
[]
["192.168.1.150","号牌机",1,"号牌机ip区域150-159，未使用部分留作备用"]
["192.168.1.151",null,2]
["192.168.1.152",null,3]
["192.168.1.153",null,4]
["192.168.1.154",null,5]
["192.168.1.155",null,6]
[]
["192.168.1.160","LED方屏",1,"入口LED屏ip区域160-179，方屏长屏顺序排布，剩余ip留作备用"]
["192.168.1.161",null,2]
["192.168.1.162",null,3]
["192.168.1.163",null,4]
["192.168.1.164",null,5]
["192.168.1.165",null,6]
["192.168.1.166","LED长屏",1]
["192.168.1.167",null,2]
["192.168.1.168",null,3]
["192.168.1.169","LED取车屏"]
[]
["192.168.1.180","终端 入口",1,"终端ip区域180-189，剩余ip备用"]
["192.168.1.181",null,2]
["192.168.1.182",null,3]
["192.168.1.183",null,4]
["192.168.1.184",null,5]
["192.168.1.185",null,6]
["192.168.1.186","终端 出口",1]
["192.168.1.187",null,2]
[]
["192.168.1.201:2368","多线雷达",7,"入口投影仪ip区域190-199，剩余ip备用"]
["192.168.1.202:2369",null,6]
["192.168.1.203:2370",null,5]
["192.168.1.204:2371",null,4]
["192.168.1.205:2372",null,3]
["192.168.1.206:2373",null,2]
["192.168.1.207:2374",null,1]
[]
["192.168.1.233","主控电脑",1]
[]
["192.168.1.239","监控电脑",1,"多线雷达ip区域201-210，剩余ip备用"]
[]
["192.168.1.240","调试设备",1]
[]
[]
[]
[]
[]
[null,null,null,"主控电脑唯一。该ip下包含节点有：主控（端口30000）、调度（30030-30032）、车位管理（端口30008）、地面测量（30010）、取车非标(30009)"]
[]
[null,null,null,"监控windows电脑唯一"]
[]
[null,null,null,"240-254用于临时调试设备接入"]

{"sheet":"Sheet2","index":1,"n_rows":20,"n_cols":4,"rows_kept":20,"cut":false,"hidden":false,"merged":[]}
["IP地址","设备类型","设备编号","备注"]
["192.168.0.220","Vim3控制卡","A"]
["192.168.0.221","Mid70"]
["192.168.0.222","Mid70"]
["192.168.0.223","Mid70"]
["192.168.0.224","Mid70"]
[]
["192.168.0.230","vim3控制卡","B"]
["192.168.0.231","mid70"]
["192.168.0.232","mid70"]
["192.168.0.235","mid70"]
["192.168.0.234","mid70"]
[]
["192.168.0.240","vim3控制卡","C"]
["192.168.0.241","mid70"]
["192.168.0.242","mid70"]
["192.168.0.243","mid70"]
["192.168.0.244","mid70"]
[]
["192.168.0.249","主控"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}