{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["A库（81-160）","B库（161-240）","C库（1-70）"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"A库（81-160）","index":0,"n_rows":33,"n_cols":3,"rows_kept":33,"cut":false,"hidden":false,"merged":[[1,0,3,0],[4,0,5,0],[7,0,13,0],[14,0,27,0],[28,0,32,0]]}
["类型","设备名称","IP地址"]
["CPU","CPU 1515-2 PN","192.168.0.81"]
[null,"CPU 1214C DC/DC/DC","192.168.0.82"]
[null,"CPU 1511-1 PN","192.168.0.111"]
["HMI","HMI KTP400","192.168.0.112"]
[null,"HMI KTP1200","192.168.0.87"]
["交换机","EKI-5526-PN","192.168.0.91"]
["IO","C3远程模块","192.168.0.101"]
[null,"C4远程模块","192.168.0.102"]
[null,"C5远程模块","192.168.0.103"]
[null,"C6远程模块","192.168.0.104"]
[null,"X轴激光模块","192.168.0.105"]
[null,"Z轴激光模块","192.168.0.114"]
[null,"Z轴远程模块","192.168.0.115"]
["驱动","Z","192.168.0.113"]
[null,"B1","192.168.0.121"]
[null,"B2","192.168.0.122"]
[null,"C3","192.168.0.123"]
[null,"C4","192.168.0.124"]
[null,"C5","192.168.0.125"]
[null,"C6","192.168.0.126"]
[null,"X","192.168.0.127"]
[null,"Y1","192.168.0.128"]
[null,"Y2","192.168.0.129"]
[null,"Y3","192.168.0.130"]
[null,"Y4","192.168.0.131"]
[null,"Y5","192.168.0.132"]
[null,"Y6","192.168.0.133"]
["安全系统","控制板","192.168.0.220"]
[null,"入口雷达1","192.168.0.221"]
[null,"入口雷达2","192.168.0.222"]
[null,"出口雷达1","192.168.0.223"]
[null,"出口雷达2","192.168.0.224"]

{"sheet":"B库（161-240）","index":1,"n_rows":33,"n_cols":3,"rows_kept":33,"cut":false,"hidden":false,"merged":[[1,0,3,0],[4,0,5,0],[7,0,13,0],[14,0,27,0],[28,0,32,0]]}
["类型","设备名称","IP地址"]
["CPU","CPU 1515-2 PN","192.168.0.161"]
[null,"CPU 1214C DC/DC/DC","192.168.0.162"]
[null,"CPU 1511-1 PN","192.168.0.191"]
["HMI","HMI KTP400","192.168.0.192"]
[null,"HMI KTP1200","192.168.0.167"]
["交换机","EKI-5526-PN","192.168.0.171"]
["IO","C3远程模块","192.168.0.181"]
[null,"C4远程模块","192.168.0.182"]
[null,"C5远程模块","192.168.0.183"]
[null,"C6远程模块","192.168.0.184"]
[null,"X轴激光模块","192.168.0.185"]
[null,"Z轴激光模块","192.168.0.194"]
[null,"Z轴远程模块","192.168.0.195"]
["驱动","Z","192.168.0.193"]
[null,"B1","192.168.0.201"]
[null,"B2","192.168.0.202"]
[null,"C3","192.168.0.203"]
[null,"C4","192.168.0.204"]
[null,"C5","192.168.0.205"]
[null,"C6","192.168.0.206"]
[null,"X","192.168.0.207"]
[null,"Y1","192.168.0.208"]
[null,"Y2","192.168.0.209"]
[null,"Y3","192.168.0.210"]
[null,"Y4","192.168.0.211"]
[null,"Y5","192.168.0.212"]
[null,"Y6","192.168.0.213"]
["安全系统","控制板","192.168.0.230"]
[null,"入口雷达1","192.168.0.231"]
[null,"入口雷达2","192.168.0.232"]
[null,"出口雷达1","192.168.0.233"]
[null,"出口雷达2","192.168.0.234"]

{"sheet":"C库（1-70）","index":2,"n_rows":33,"n_cols":3,"rows_kept":33,"cut":false,"hidden":false,"merged":[[1,0,3,0],[4,0,5,0],[7,0,13,0],[14,0,27,0],[28,0,32,0]]}
["类型","设备名称","IP地址"]
["CPU","CPU 1515-2 PN","192.168.0.1"]
[null,"CPU 1214C DC/DC/DC","192.168.0.30"]
[null,"CPU 1511-1 PN","192.168.0.51"]
["HMI","HMI KTP400","192.168.0.52"]
[null,"HMI KTP1200","192.168.0.21"]
["交换机","EKI-5526-PN","192.168.0.3"]
["IO","C3远程模块","192.168.0.15"]
[null,"C4远程模块","192.168.0.16"]
[null,"C5远程模块","192.168.0.17"]
[null,"C6远程模块","192.168.0.18"]
[null,"X轴激光模块","192.168.0.19"]
[null,"Z轴激光模块","192.168.0.54"]
[null,"Z轴远程模块","192.168.0.55"]
["驱动","Z","192.168.0.53"]
[null,"B1","192.168.0.19"]
[null,"B2","192.168.0.20"]
[null,"C3","192.168.0.10"]
[null,"C4","192.168.0.11"]
[null,"C5","192.168.0.12"]
[null,"C6","192.168.0.13"]
[null,"X","192.168.0.2"]
[null,"Y1","192.168.0.3"]
[null,"Y2","192.168.0.4"]
[null,"Y3","192.168.0.5"]
[null,"Y4","192.168.0.6"]
[null,"Y5","192.168.0.7"]
[null,"Y6","192.168.0.8"]
["安全系统","控制板","192.168.0.240"]
[null,"入口雷达1","192.168.0.241"]
[null,"入口雷达2","192.168.0.242"]
[null,"出口雷达1","192.168.0.243"]
[null,"出口雷达2","192.168.0.244"]